,Model##OTHER##,Total System Weight##OTHER##,Voltage Input Output Comment##OTHER##,Input Voltage##ELECTRICAL_POTENTIAL##VOLTS
Illuminator Supernova Inverter System - 120-120 Volts - 10.0 KVA - Standard Cabinet - 120 Min Runtime,1-I-10-S-R120,2404 lbs,120-120 Volts,120
Illuminator Supernova Inverter System - 120-120 Volts - 10.0 KVA - Standard Cabinet - 90 Min Runtime,1-I-10-S,2404 lbs,120-120 Volts,120
Illuminator Supernova Inverter System - 120-120 Volts - 12.5 KVA - Standard Cabinet - 120 Min Runtime,1-I-12-S-R120,2810 lbs,120-120 Volts,120
Illuminator Supernova Inverter System - 120-120 Volts - 12.5 KVA - Standard Cabinet - 90 Min Runtime,1-I-12-S,2810 lbs,120-120 Volts,120
Illuminator Supernova Inverter System - 120-120 Volts - 16.7 KVA - Standard Cabinet - 120 Min Runtime,1-I-16-S-R120,3470 lbs,120-120 Volts,120
Illuminator Supernova Inverter System - 120-120 Volts - 16.7 KVA - Standard Cabinet - 90 Min Runtime,1-I-16-S,3470 lbs,120-120 Volts,120
Illuminator Supernova Inverter System - 120-120/277 Volts - 10.0 KVA - Standard Cabinet - 120 Min Runtime,2-I-10-S-R120,2404 lbs,120-120/277 Volts,120
Illuminator Supernova Inverter System - 120-120/277 Volts - 10.0 KVA - Standard Cabinet - 90 Min Runtime,2-I-10-S,2404 lbs,120-120/277 Volts,120
Illuminator Supernova Inverter System - 120-120/277 Volts - 12.5 KVA - Standard Cabinet - 120 Min Runtime,2-I-12-S-R120,2810 lbs,120-120/277 Volts,120
Illuminator Supernova Inverter System - 120-120/277 Volts - 12.5 KVA - Standard Cabinet - 90 Min Runtime,2-I-12-S,2810 lbs,120-120/277 Volts,120
Illuminator Supernova Inverter System - 120-120/277 Volts - 16.7 KVA - Standard Cabinet - 120 Min Runtime,2-I-16-S-R120,3470 lbs,120-120/277 Volts,120
Illuminator Supernova Inverter System - 120-120/277 Volts - 16.7 KVA - Standard Cabinet - 90 Min Runtime,2-I-16-S,3470 lbs,120-120/277 Volts,120
Illuminator Supernova Inverter System - 208-120 Volts - 10.0 KVA - Standard Cabinet - 120 Min Runtime,3-I-10-S-R120,2404 lbs,208-120 Volts,208
Illuminator Supernova Inverter System - 208-120 Volts - 10.0 KVA - Standard Cabinet - 90 Min Runtime,3-I-10-S,2404 lbs,208-120 Volts,208
Illuminator Supernova Inverter System - 208-120 Volts - 12.5 KVA - Standard Cabinet - 120 Min Runtime,3-I-12-S-R120,2810 lbs,208-120 Volts,208
Illuminator Supernova Inverter System - 208-120 Volts - 12.5 KVA - Standard Cabinet - 90 Min Runtime,3-I-12-S,2810 lbs,208-120 Volts,208
Illuminator Supernova Inverter System - 208-120 Volts - 16.7 KVA - Standard Cabinet - 120 Min Runtime,3-I-16-S-R120,3470 lbs,208-120 Volts,208
Illuminator Supernova Inverter System - 208-120 Volts - 16.7 KVA - Standard Cabinet - 90 Min Runtime,3-I-16-S,3470 lbs,208-120 Volts,208
Illuminator Supernova Inverter System - 240-120/240 Volts - 10.0 KVA - Standard Cabinet - 120 Min Runtime,4-I-10-S-R120,2404 lbs,240-120/240 Volts,240
Illuminator Supernova Inverter System - 240-120/240 Volts - 10.0 KVA - Standard Cabinet - 90 Min Runtime,4-I-10-S,2404 lbs,240-120/240 Volts,240
Illuminator Supernova Inverter System - 240-120/240 Volts - 12.5 KVA - Standard Cabinet - 120 Min Runtime,4-I-12-S-R120,2810 lbs,240-120/240 Volts,240
Illuminator Supernova Inverter System - 240-120/240 Volts - 12.5 KVA - Standard Cabinet - 90 Min Runtime,4-I-12-S,2810 lbs,240-120/240 Volts,240
Illuminator Supernova Inverter System - 240-120/240 Volts - 16.7 KVA - Standard Cabinet - 120 Min Runtime,4-I-16-S-R120,3470 lbs,240-120/240 Volts,240
Illuminator Supernova Inverter System - 240-120/240 Volts - 16.7 KVA - Standard Cabinet - 90 Min Runtime,4-I-16-S,3470 lbs,240-120/240 Volts,240
Illuminator Supernova Inverter System - 277-120 Volts - 10.0 KVA - Standard Cabinet - 120 Min Runtime,5-I-10-S-R120,2404 lbs,277-120 Volts,277
Illuminator Supernova Inverter System - 277-120 Volts - 10.0 KVA - Standard Cabinet - 90 Min Runtime,5-I-10-S,2404 lbs,277-120 Volts,277
Illuminator Supernova Inverter System - 277-120 Volts - 12.5 KVA - Standard Cabinet - 120 Min Runtime,5-I-12-S-R120,2810 lbs,277-120 Volts,277
Illuminator Supernova Inverter System - 277-120 Volts - 12.5 KVA - Standard Cabinet - 90 Min Runtime,5-I-12-S,2810 lbs,277-120 Volts,277
Illuminator Supernova Inverter System - 277-120 Volts - 16.7 KVA - Standard Cabinet - 120 Min Runtime,5-I-16-S-R120,3470 lbs,277-120 Volts,277
Illuminator Supernova Inverter System - 277-120 Volts - 16.7 KVA - Standard Cabinet - 90 Min Runtime,5-I-16-S,3470 lbs,277-120 Volts,277
Illuminator Supernova Inverter System - 277-277 Volts - 10.0 KVA - Standard Cabinet - 120 Min Runtime,6-I-10-S-R120,2404 lbs,277-277 Volts,277
Illuminator Supernova Inverter System - 277-277 Volts - 10.0 KVA - Standard Cabinet - 90 Min Runtime,6-I-10-S,2404 lbs,277-277 Volts,277
Illuminator Supernova Inverter System - 277-277 Volts - 12.5 KVA - Standard Cabinet - 120 Min Runtime,6-I-12-S-R120,2810 lbs,277-277 Volts,277
Illuminator Supernova Inverter System - 277-277 Volts - 12.5 KVA - Standard Cabinet - 90 Min Runtime,6-I-12-S,2810 lbs,277-277 Volts,277
Illuminator Supernova Inverter System - 277-277 Volts - 16.7 KVA - Standard Cabinet - 120 Min Runtime,6-I-16-S-R120,3470 lbs,277-277 Volts,277
Illuminator Supernova Inverter System - 277-277 Volts - 16.7 KVA - Standard Cabinet - 90 Min Runtime,6-I-16-S,3470 lbs,277-277 Volts,277
Illuminator Supernova Inverter System - 277-277/120 Volts - 10.0 KVA - Standard Cabinet - 120 Min Runtime,7-I-10-S-R120,2404 lbs,277-277/120 Volts,277
Illuminator Supernova Inverter System - 277-277/120 Volts - 10.0 KVA - Standard Cabinet - 90 Min Runtime,7-I-10-S,2404 lbs,277-277/120 Volts,277
Illuminator Supernova Inverter System - 277-277/120 Volts - 12.5 KVA - Standard Cabinet - 120 Min Runtime,7-I-12-S-R120,2810 lbs,277-277/120 Volts,277
Illuminator Supernova Inverter System - 277-277/120 Volts - 12.5 KVA - Standard Cabinet - 90 Min Runtime,7-I-12-S,2810 lbs,277-277/120 Volts,277
Illuminator Supernova Inverter System - 277-277/120 Volts - 16.7 KVA - Standard Cabinet - 120 Min Runtime,7-I-16-S-R120,3470 lbs,277-277/120 Volts,277
Illuminator Supernova Inverter System - 277-277/120 Volts - 16.7 KVA - Standard Cabinet - 90 Min Runtime,7-I-16-S,3470 lbs,277-277/120 Volts,277
Illuminator Supernova Inverter System - 208-120/240 Volts - 10.0 KVA - Standard Cabinet - 120 Min Runtime,8-I-10-S-R120,2404 lbs,208-120/240 Volts,208
Illuminator Supernova Inverter System - 208-120/240 Volts - 10.0 KVA - Standard Cabinet - 90 Min Runtime,8-I-10-S,2404 lbs,208-120/240 Volts,208
Illuminator Supernova Inverter System - 208-120/240 Volts - 12.5 KVA - Standard Cabinet - 120 Min Runtime,8-I-12-S-R120,2810 lbs,208-120/240 Volts,208
Illuminator Supernova Inverter System - 208-120/240 Volts - 12.5 KVA - Standard Cabinet - 90 Min Runtime,8-I-12-S,2810 lbs,208-120/240 Volts,208
Illuminator Supernova Inverter System - 208-120/240 Volts - 16.7 KVA - Standard Cabinet - 120 Min Runtime,8-I-16-S-R120,3470 lbs,208-120/240 Volts,208
Illuminator Supernova Inverter System - 208-120/240 Volts - 16.7 KVA - Standard Cabinet - 90 Min Runtime,8-I-16-S,3470 lbs,208-120/240 Volts,208
Illuminator Supernova Inverter System - 208-120/208 Volts - 10.0 KVA - Standard Cabinet - 120 Min Runtime,A-I-10-S-R120,2404 lbs,208-120/208 Volts,208
Illuminator Supernova Inverter System - 208-120/208 Volts - 10.0 KVA - Standard Cabinet - 90 Min Runtime,A-I-10-S,2404 lbs,208-120/208 Volts,208
Illuminator Supernova Inverter System - 208-120/208 Volts - 12.5 KVA - Standard Cabinet - 120 Min Runtime,A-I-12-S-R120,2810 lbs,208-120/208 Volts,208
Illuminator Supernova Inverter System - 208-120/208 Volts - 12.5 KVA - Standard Cabinet - 90 Min Runtime,A-I-12-S,2810 lbs,208-120/208 Volts,208
Illuminator Supernova Inverter System - 208-120/208 Volts - 16.7 KVA - Standard Cabinet - 120 Min Runtime,A-I-16-S-R120,3470 lbs,208-120/208 Volts,208
Illuminator Supernova Inverter System - 208-120/208 Volts - 16.7 KVA - Standard Cabinet - 90 Min Runtime,A-I-16-S,3470 lbs,208-120/208 Volts,208
