,Model##OTHER##,Total System Weight##OTHER##,Voltage Input Output Comment##OTHER##,Input Voltage##ELECTRICAL_POTENTIAL##VOLTS
Illuminator Supernova Inverter System - 120-120 Volts - 6.25 KVA - Standard Cabinet - 120 Min Runtime,1-I-06-S-R120,1618 lbs,120-120 Volts,120
Illuminator Supernova Inverter System - 120-120 Volts - 6.25 KVA - Standard Cabinet - 90 Min Runtime,1-I-06-S,1618 lbs,120-120 Volts,120
Illuminator Supernova Inverter System - 120-120 Volts - 7.5 KVA - Standard Cabinet - 120 Min Runtime,1-I-07-S-R120,1884 lbs,120-120 Volts,120
Illuminator Supernova Inverter System - 120-120 Volts - 7.5 KVA - Standard Cabinet - 90 Min Runtime,1-I-07-S,1884 lbs,120-120 Volts,120
Illuminator Supernova Inverter System - 120-120/277 Volts - 6.25 KVA - Standard Cabinet - 120 Min Runtime,2-I-06-S-R120,1618 lbs,120-120/277 Volts,120
Illuminator Supernova Inverter System - 120-120/277 Volts - 6.25 KVA - Standard Cabinet - 90 Min Runtime,2-I-06-S,1618 lbs,120-120/277 Volts,120
Illuminator Supernova Inverter System - 120-120/277 Volts - 7.5 KVA - Standard Cabinet - 120 Min Runtime,2-I-07-S-R120,1884 lbs,120-120/277 Volts,120
Illuminator Supernova Inverter System - 120-120/277 Volts - 7.5 KVA - Standard Cabinet - 90 Min Runtime,2-I-07-S,1884 lbs,120-120/277 Volts,120
Illuminator Supernova Inverter System - 208-120 Volts - 6.25 KVA - Standard Cabinet - 120 Min Runtime,3-I-06-S-R120,1618 lbs,208-120 Volts,208
Illuminator Supernova Inverter System - 208-120 Volts - 6.25 KVA - Standard Cabinet - 90 Min Runtime,3-I-06-S,1618 lbs,208-120 Volts,208
Illuminator Supernova Inverter System - 208-120 Volts - 7.5 KVA - Standard Cabinet - 120 Min Runtime,3-I-07-S-R120,1884 lbs,208-120 Volts,208
Illuminator Supernova Inverter System - 208-120 Volts - 7.5 KVA - Standard Cabinet - 90 Min Runtime,3-I-07-S,1884 lbs,208-120 Volts,208
Illuminator Supernova Inverter System - 240-120/240 Volts - 6.25 KVA - Standard Cabinet - 120 Min Runtime,4-I-06-S-R120,1618 lbs,240-120/240 Volts,240
Illuminator Supernova Inverter System - 240-120/240 Volts - 6.25 KVA - Standard Cabinet - 90 Min Runtime,4-I-06-S,1618 lbs,240-120/240 Volts,240
Illuminator Supernova Inverter System - 240-120/240 Volts - 7.5 KVA - Standard Cabinet - 120 Min Runtime,4-I-07-S-R120,1884 lbs,240-120/240 Volts,240
Illuminator Supernova Inverter System - 240-120/240 Volts - 7.5 KVA - Standard Cabinet - 90 Min Runtime,4-I-07-S,1884 lbs,240-120/240 Volts,240
Illuminator Supernova Inverter System - 277-120 Volts - 6.25 KVA - Standard Cabinet - 120 Min Runtime,5-I-06-S-R120,1618 lbs,277-120 Volts,277
Illuminator Supernova Inverter System - 277-120 Volts - 6.25 KVA - Standard Cabinet - 90 Min Runtime,5-I-06-S,1618 lbs,277-120 Volts,277
Illuminator Supernova Inverter System - 277-120 Volts - 7.5 KVA - Standard Cabinet - 120 Min Runtime,5-I-07-S-R120,1884 lbs,277-120 Volts,277
Illuminator Supernova Inverter System - 277-120 Volts - 7.5 KVA - Standard Cabinet - 90 Min Runtime,5-I-07-S,1884 lbs,277-120 Volts,277
Illuminator Supernova Inverter System - 277-277 Volts - 6.25 KVA - Standard Cabinet - 120 Min Runtime,6-I-06-S-R120,1618 lbs,277-277 Volts,277
Illuminator Supernova Inverter System - 277-277 Volts - 6.25 KVA - Standard Cabinet - 90 Min Runtime,6-I-06-S,1618 lbs,277-277 Volts,277
Illuminator Supernova Inverter System - 277-277 Volts - 7.5 KVA - Standard Cabinet - 120 Min Runtime,6-I-07-S-R120,1884 lbs,277-277 Volts,277
Illuminator Supernova Inverter System - 277-277 Volts - 7.5 KVA - Standard Cabinet - 90 Min Runtime,6-I-07-S,1884 lbs,277-277 Volts,277
Illuminator Supernova Inverter System - 277-277/120 Volts - 6.25 KVA - Standard Cabinet - 120 Min Runtime,7-I-06-S-R120,1618 lbs,277-277/120 Volts,277
Illuminator Supernova Inverter System - 277-277/120 Volts - 6.25 KVA - Standard Cabinet - 90 Min Runtime,7-I-06-S,1618 lbs,277-277/120 Volts,277
Illuminator Supernova Inverter System - 277-277/120 Volts - 7.5 KVA - Standard Cabinet - 120 Min Runtime,7-I-07-S-R120,1884 lbs,277-277/120 Volts,277
Illuminator Supernova Inverter System - 277-277/120 Volts - 7.5 KVA - Standard Cabinet - 90 Min Runtime,7-I-07-S,1884 lbs,277-277/120 Volts,277
Illuminator Supernova Inverter System - 208-120/240 Volts - 6.25 KVA - Standard Cabinet - 120 Min Runtime,8-I-06-S-R120,1618 lbs,208-120/240 Volts,208
Illuminator Supernova Inverter System - 208-120/240 Volts - 6.25 KVA - Standard Cabinet - 90 Min Runtime,8-I-06-S,1618 lbs,208-120/240 Volts,208
Illuminator Supernova Inverter System - 208-120/240 Volts - 7.5 KVA - Standard Cabinet - 120 Min Runtime,8-I-07-S-R120,1884 lbs,208-120/240 Volts,208
Illuminator Supernova Inverter System - 208-120/240 Volts - 7.5 KVA - Standard Cabinet - 90 Min Runtime,8-I-07-S,1884 lbs,208-120/240 Volts,208
Illuminator Supernova Inverter System - 208-120/208 Volts - 6.25 KVA - Standard Cabinet - 120 Min Runtime,A-I-06-S-R120,1618 lbs,208-120/208 Volts,208
Illuminator Supernova Inverter System - 208-120/208 Volts - 6.25 KVA - Standard Cabinet - 90 Min Runtime,A-I-06-S,1618 lbs,208-120/208 Volts,208
Illuminator Supernova Inverter System - 208-120/208 Volts - 7.5 KVA - Standard Cabinet - 120 Min Runtime,A-I-07-S-R120,1884 lbs,208-120/208 Volts,208
Illuminator Supernova Inverter System - 208-120/208 Volts - 7.5 KVA - Standard Cabinet - 90 Min Runtime,A-I-07-S,1884 lbs,208-120/208 Volts,208
